{"text_format":"5","workbook":"xlsx","n_sheets":1,"sheets":["전체"],"props":{"creator":"김태환","last_modified_by":"user"},"not_rendered":{"defined_names":1},"read":"whole","date_system":"1900"}

{"sheet":"전체","index":0,"n_rows":16,"n_cols":68,"rows_kept":16}
["No.","국가코드","발명의 명칭","요약","독립항","출원인","발명자","문헌종류 코드","출원번호","출원일","등록번호","메인 IPC","우선권 국가","우선권 번호","우선권 주장일","특허/실용구분","대표청구항","요약(원문)","청구항 수","법적상태","심사청구여부(KR,JP,EP)","심사진행상태","출원인 국적","현재권리자","현재권리자 국적","발명자(원문)","발명자 국적","대리인","공개번호","공개일","등록일","심사청구일(KR,JP,EP)","존속기간 만료일","원출원번호","원출원일자","공개/등록번호 ","공개/등록일자 ","전체 IPC","메인 CPC","전체 CPC","FI (File Index)","메인 US Class","전체 US Class","테마코드(JP)","F-Term(JP)","최우선일","국제출원번호","국제출원일","국제공개번호","국제공개일","번역문제출일(KR)","인용문헌번호","인용문헌수","국가별 인용문헌수","인용문헌국가","자국인용문헌번호","심사관인용문헌(KR,US)","피인용문헌번호","피인용문헌수","국가별 피인용문헌수","피인용문헌국가","패밀리 국가수","패밀리 문헌수","패밀리 문헌번호","패밀리 국가별 문헌수","EPO심플패밀리 문헌번호","EPO심플패밀리 문헌수","EPO심플패밀리 국가별 문헌수"]
[1,"KR","Iot를 기반 스마트 센서를 포함하는 환자 상태 실시간 정보 전송 시스템(real-time information transmission system to patient status including smart sensor based on internet of things)","본 발명은 IoT를 기반 스마트 센서를 포함하는 환자 상태 실시간 정보 전송 시스템에 관한 것이다. 보다 구체적으로, 지능형 인지 프레임워크를 사용하여 환자 상태 모니터링 및 헬스 케어가 가능하도록 스마트 센서 연결 계층 구조와 서비스 연결되어 웹 서비스에서 상기 스마트 센서에 대한 실시간 반응하는 IoT 브로커를 통해 정형화된 센싱 데이터, 멀티 프로토콜 자동 선택이 가능하도록 응급 수송차량에 의료장비 통신모듈이 구비된 IoT를 기반 스마트 센서를 포함하는 환자 상태 실시간 정보 전송 시스템에 관한 것이다. 본 발명에 따른 IoT를 기반 스마트 센서를 포함하는 환자 상태 실시간 정보 전송 시스템은, 센서 연결 계층 구조와 서비스 연결되어 웹 서비스에서 센서에 대한 실시간 반응하는 IoT 브로커를 통해 정형화된 센싱 데이터, 멀티 프로토콜 자동 선택이 가능하도록 응급 수송차량에 의료장비 통신 모듈을 통해 지능형 인지 프레임워크를 사용하여 환자 상태 모니터링 및 헬스케어가 가능한 효과를 제공할 수 있다. 또한, 본 발명에 따른 IoT를 기반 스마트 센서를 포함하는 환자 상태 실시간 정보 전송 시스템은, 응급 수송차량에 의료장비에 설치할 수 있는 통신 모듈을 통해 실시간 응급환자의 상태 체크, 응급처치가 가능하고 응급 차량 내에서 환자의 바이탈 신호를 의료진에게 신속히 전송할 수 있고, 상황 인지 프레임워크와 개방형 서비스 플랫폼을 사용하여 환자의 상황을 의료진의 판단과 함께 시스템에서 위험도를 예측하여 사전 예방 조치를 취할 수 있는 효과를 제공할 수 있다.","[청구항1]\nIoT를 기반 스마트 센서를 포함하는 환자 상태 실시간 정보 전송 시스템에 있어서,\n상기 시스템은 웹 서비스에서 센서에 대한 정확성을 제공하고 정형화된 센싱 데이터 및 명령어 제공, 멀티 프로토콜 자동 선택과 처리가 가능하여 센서 및 제어기 연동이 가능하여 보안 및 안정성 강화를 제공되는 IoT 브로커; 및\n센서노드와 무선으로 연동되어, 센서노드에서 전송되는 정형화된 센싱데이터 및 명령어를 IoT 응용 서비스로 멀티 프로토콜 자동 선택 및 처리를 통해 보안 및 프라이버시 강화하여 환자 상태 판단시 지능형 인지 프레임워크를 사용하여 환자 상태 모니터링 및 헬스케어가 가능하도록 센서 연결 계층 구조와 서비스 연결되어 웹 서비스에서 센서에 대한 실시간 반응하는 IoT 브로커를 통해 정형화된 센싱 데이터, 멀티 프로토콜 자동 선택이 가능하도록 제어부를 포함하는 것을 특징으로 하는 IoT를 기반 스마트 센서를 포함하는 환자 상태 실시간 정보 전송 시스템.","주식회사 에스엠디솔루션","김현정","A","2018-0138327","2018.11.12","-","A61B-005/00","-","-","-","특허공개","[청구항1]\n IoT를 기반 스마트 센서를 포함하는 환자 상태 실시간 정보 전송 시스템에 있어서,\n상기 시스템은 웹 서비스에서 센서에 대한 정확성을 제공하고 정형화된 센싱 데이터 및 명령어 제공, 멀티 프로토콜 자동 선택과 처리가 가능하여 센서 및 제어기 연동이 가능하여 보안 및 안정성 강화를 제공되는 IoT 브로커; 및\n센서노드와 무선으로 연동되어, 센서노드에서 전송되는 정형화된 센싱데이터 및 명령어를 IoT 응용 서비스로 멀티 프로토콜 자동 선택 및 처리를 통해 보안 및 프라이버시 강화하여 환자 상태 판단시 지능형 인지 프레임워크를 사용하여 환자 상태 모니터링 및 헬스케어가 가능하도록 센서 연결 계층 구조와 서비스 연결되어 웹 서비스에서 센서에 대한 실시간 반응하는 IoT 브로커를 통해 정형화된 센싱 데이터, 멀티 프로토콜 자동 선택이 가능하도록 제어부를 포함하는 것을 특징으로 하는 IoT를 기반 스마트 센서를 포함하는 환자 상태 실시간 정보 전송 시스템.","-",3,"공개","N","-","KR","-","-","-","-","서상덕, 이창재","2019-0032258","2019.03.27","-","-","-","-","-","2019-0032258","2019.03.27","A61B-005/00,[A61B-005/01, A61B-005/021, A61B-005/024, A61B-005/08, A61B-005/1455]","A61B-0005/0002","A61B-0005/0002, A61B-0005/0001, A61B-0005/0021, A61B-0005/0024, A61B-0005/0008, A61B-0005/14551, A61B-0005/6831, A61B-0005/7235, A61B-0005/7275, A61B-2562/0219","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",1,1,"KR20190032258A","KR(1)","KR20190032258A",1,"KR(1)"]
[2,"KR","7세주기 기반의 피부관리 카운셀링 시스템(skincare counselling system based on 7 year aging cycle)","본 발명은 피부관리 카운셀링 시스템에 관한 것으로서, 보다 상세하게는 사용자의 피부 고민에 따라 생활 관리 및 피부관리 정보를 포함하는 맞춤 피부관리 솔루션을 제공하는 7세주기 기반의 피부관리 카운셀링 시스템에 관한 것이다.\n본 발명에 따르면, 사용자의 피부 상태를 영양, 안색 및 주름의 주 고민 항목별로 분류하여 분석함으로써, 복합적으로 피부관리 정보를 제공할 수 있고, 사용자의 피부 상태 분석 결과 데이터와 생활 양식 분석 결과를 모두 반영하여, 기후, 환경, 정신적 스트레스, 라이프스타일 등 피부 상태에 영향을 줄 수 있는 다양한 요인을 고려한 맞춤 피부관리 솔루션을 제공할 수 있다.\n또한, 본 발명에 따르면, 피부 상태가 급변하게 되는 변곡주기에 해당하는 7세 주기에 따른 연령대별 피부 고민을 고려하여 솔루션 데이터를 생성하고, 이를 사용자의 피부 상태 분석 결과 데이터와 매칭함으로써, 사용자의 피부 상태에 대한 보다 정확한 맞춤 피부관리 솔루션을 제공할 수 있다.\n또한, 본 발명에 따르면, 본 발명에 따른 피부관리 카운셀링 시스템을 이용하여, 미리 설정된 피부 고민 변곡주기에 기반한 피부관리 솔루션을 제안하는 방법을 제공할 수 있다.","[청구항1]\n데이터베이스, 피부관리 서버, 정보 입력 단말 및 사용자 단말을 포함하는 피부관리 카운셀링 시스템으로서,\n상기 피부관리 서버로부터 수신하는 사용자의 피부 상태 데이터 및 생활 양식 데이터를 포함하는 개인 정보 데이터 및 솔루션 데이터를 저장하는 데이터베이스;\n상기 데이터베이스, 정보 입력 단말 및 사용자 단말과 통신 가능하도록 연결되며, 데이터를 송수신할 수 있는 데이터 송수신부, 상기 데이터 송수신부에서 수신하는 상기 사용자의 피부 상태 데이터를 피부 고민 항목별로 분류하여 사용자의 피부 상태 분석 결과 데이터를 생성하는 피부 상태 분석부, 상기 데이터 송수신부에서 수신하는 상기 생활 양식 데이터에 따라 상기 사용자의 생활 양식 분석 결과 데이터를 생성하는 생활 양식 분석부, 상기 피부 상태 분석 결과 데이터 및 상기 생활 양식 분석 결과 데이터에 맞게 상기 솔루션 데이터를 이용하여 사용자별 맞춤 피부관리 솔루션을 생성하는 솔루션 생성부를 포함하는 피부관리 서버;\n상기 피부관리 서버와 통신 가능하도록 연결되며, 사용자의 개인 정보 데이터를 입력 받는 정보 입력 단말; 및\n상기 피부관리 서버와 통신 가능하도록 연결되며, 상기 솔루션 생성부에서 생성된 맞춤 피부관리 솔루션을 출력 가능한 사용자 단말을 포함하는 것을 특징으로 하는, 미리 설정된 피부 고민 변곡주기 기반의 피부관리 카운셀링 시스템.\n[청구항16]\n제1항 내지 제15항 중 어느 한 항에 기재된 피부관리 카운셀링 시스템을 이용하여, 미리 설정된 피부 고민 변곡주기에 기반한 피부관리 솔루션을 제안하는 방법.","(주)아모레퍼시픽","조가영 | 권이경 | 김민숙 | 최소웅 | 서병휘 | 조성아","A","2018-0114281","2018.09.21","-","G06Q-050/10","대한민국(KR)","1020170126938 ","2017.09.29","특허공개","[청구항1]\n 데이터베이스, 피부관리 서버, 정보 입력 단말 및 사용자 단말을 포함하는 피부관리 카운셀링 시스템으로서,\n상기 피부관리 서버로부터 수신하는 사용자의 피부 상태 데이터 및 생활 양식 데이터를 포함하는 개인 정보 데이터 및 솔루션 데이터를 저장하는 데이터베이스;\n상기 데이터베이스, 정보 입력 단말 및 사용자 단말과 통신 가능하도록 연결되며, 데이터를 송수신할 수 있는 데이터 송수신부, 상기 데이터 송수신부에서 수신하는 상기 사용자의 피부 상태 데이터를 피부 고민 항목별로 분류하여 사용자의 피부 상태 분석 결과 데이터를 생성하는 피부 상태 분석부, 상기 데이터 송수신부에서 수신하는 상기 생활 양식 데이터에 따라 상기 사용자의 생활 양식 분석 결과 데이터를 생성하는 생활 양식 분석부, 상기 피부 상태 분석 결과 데이터 및 상기 생활 양식 분석 결과 데이터에 맞게 상기 솔루션 데이터를 이용하여 사용자별 맞춤 피부관리 솔루션을 생성하는 솔루션 생성부를 포함하는 피부관리 서버;\n상기 피부관리 서버와 통신 가능하도록 연결되며, 사용자의 개인 정보 데이터를 입력 받는 정보 입력 단말; 및\n상기 피부관리 서버와 통신 가능하도록 연결되며, 상기 솔루션 생성부에서 생성된 맞춤 피부관리 솔루션을 출력 가능한 사용자 단말을 포함하는 것을 특징으로 하는, 미리 설정된 피부 고민 변곡주기 기반의 피부관리 카운셀링 시스템.","-",16,"공개","Y","-","KR","-","-","-","-","윤앤리특허법인(유한)","2019-0038375","2019.04.08","-","2020.03.10","-","-","-","2019-0038375","2019.04.08","G06Q-050/10","G06Q-0050/0010","G06Q-0050/0010","-","-","-","-","-","2017.09.29","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",1,1,"KR20190038375A","KR(1)","KR20190038375A",1,"KR(1)"]
[3,"KR","의료 중재 레벨을 원격으로 판단하기 위한 방법 및 시스템(methods and systems for remotely determining levels of healthcare interventions)","본 발명은 가능한 한 오랫동안 최저 의료 비용 설정으로 집에 환자를 유지하기 위해 \"무료인\" 손 및 눈으로부터 숙련된 임상 의사로 점진적으로 보다 높은 레벨의 의료 및 개입을 트리거링하도록 환자의 건강이 악화될 수 있는 때를 판단하기 위해 착용 가능한 센서 기술을 사용하는 방법 및 시스템에 관한 것이다.","[청구항1]\n의료 통신 시스템으로서,\n착용 가능한 센서;\n상기 센서의 착용자의 활동에 대응하는 상태 정보를 상기 센서로부터 무선으로 수신하기 위한 로컬(local) 통신 시스템;\n상기 로컬 통신 시스템과 통신을 행하는 원격(remote) 서버; 및\n상태 정보와 이벤트에 응답하여 취해질 행위를 저장하기 위한 데이터베이스를 포함하고,\n상기 센서, 상기 로컬 통신 시스템 또는 서버 중 적어도 하나는, (a) 상기 데이터베이스에서 타임스탬프(timestamp)된 상태 정보를 저장하여 상기 착용자의 적어도 하나의 베이스라인 활동 패턴을 확립하고, (b) 현재 상태 정보에 기초하여, 저장된 베이스라인 활동 패턴으로부터의 상기 현재 상태 정보의 변화량에 기초한 이벤트를 추론하고, (c) 상기 원격 서버가 상기 데이터베이스에서 상기 이벤트에 대응하는 행위를 수행하게 하도록 구성되는, 의료 통신 시스템.\n[청구항13]\n의료 통신 방법으로서,\n사용자가 착용한 센서로부터 사용자의 활동에 대응하는 상태 정보를 무선으로 수신하는 단계;\n상태 정보와, 사용자에게 영향을 미치는 이벤트들에 응답하여 취해질 행위를 데이터베이스에 전자적으로 저장하는 단계;\n사용자의 적어도 하나의 베이스라인 활동 패턴을 확립하는 타임스탬프된 상태 정보를 상기 데이터베이스에 전자적으로 저장하는 단계;\n현재 상태 정보에 기초하여, 저장된 베이스라인 활동 패턴으로부터 수신된 상태 정보의 변화량에 기초한 이벤트를 계산상으로(computationally) 추론하는 단계; 및\n사용자로부터의 원격 서버에 의해, 상기 데이터베이스에서 상기 이벤트에 대응하는 행위의 수행이 이루어지게 하는 단계를 포함하는, 의료 통신 방법.","케어프리딕트, 인코퍼레이티드","사티쉬 모브바","A","2018-0107630","2018.09.10","-","G06Q-050/22","미국(US)","13/896,306 ","2013.05.16","특허공개","[청구항1]\n 의료 통신 시스템으로서,\n착용 가능한 센서;\n상기 센서의 착용자의 활동에 대응하는 상태 정보를 상기 센서로부터 무선으로 수신하기 위한 로컬(local) 통신 시스템;\n상기 로컬 통신 시스템과 통신을 행하는 원격(remote) 서버; 및\n상태 정보와 이벤트에 응답하여 취해질 행위를 저장하기 위한 데이터베이스를 포함하고,\n상기 센서, 상기 로컬 통신 시스템 또는 서버 중 적어도 하나는, (a) 상기 데이터베이스에서 타임스탬프(timestamp)된 상태 정보를 저장하여 상기 착용자의 적어도 하나의 베이스라인 활동 패턴을 확립하고, (b) 현재 상태 정보에 기초하여, 저장된 베이스라인 활동 패턴으로부터의 상기 현재 상태 정보의 변화량에 기초한 이벤트를 추론하고, (c) 상기 원격 서버가 상기 데이터베이스에서 상기 이벤트에 대응하는 행위를 수행하게 하도록 구성되는, 의료 통신 시스템.","-",16,"공개","Y","-","US","-","-","-","-","황의만","2018-0103032","2018.09.18","-","2018.09.10","-","10-2018-0042187","20180411","2018-0103032","2018.09.18","G06Q-050/22,[A61B-005/00, G16H-040/40]","G06Q-0050/0022","G06Q-0050/0022, A61B-0005/6843, G16H-0040/0040","-","-","-","-","-","2013.05.16","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",4,16,"US9798860B1, CA2838232C, FR3054694A1, KR20140135591A, KR20180043765A, KR101901760B1, US2017293729A1, KR101960760B1, US9734295B1, CA2838232A1, US2018025123A1, KR20190025881A, FR3005767A1, KR20180103032A, FR3054693A1, FR3005767B1","KR(6), FR(4), US(4), CA(2)","US9798860B1, CA2838232C, FR3054694A1, KR20140135591A, KR20180043765A, KR101901760B1, US2017293729A1, KR101960760B1, US9734295B1, CA2838232A1, US2018025123A1, KR20190025881A, FR3005767A1, KR20180103032A, FR3054693A1, FR3005767B1",16,"KR(6), FR(4), US(4), CA(2)"]
[1,"US","Computer-implemented system and method for providing a personal mobile device-triggered medical intervention","A computer-implemented system and method for providing a personal mobile device-triggered medical intervention is provided. An activity monitor is associated with a patient and is configured to sense cardiac activity data, including heart rate and heart rhythm. A mobile device is paired with the activity monitor to execute an application for detecting a potentially medically significant cardiac event based on the cardiac activity data. An electrocardiography and physiological sensor monitor is fitted to a sternal region of the patient to sense electrocardiographic signals that the activity monitor is not capable of obtaining. The patient's access to the electrocardiography and physiological sensor monitor is triggered upon detection of the potentially medically significant cardiac event and the electrocardiographic signals are directly uploaded into an electronic medical record for the patient for review by a medical professional.","[청구항1]\n1. A computer-implemented system, comprising:an activity monitor associated with a patient and configured to sense cardiac activity data comprising heart rate or heart rhythm;a mobile device paired with the activity monitor to execute an application to detect a potentially medically significant cardiac event based on the cardiac activity data; andan electrocardiography and physiological sensor monitor fitted to a sternal region of the patient to sense electrocardiographic signals that the activity monitor is not capable of obtaining, wherein the patient's access to the electrocardiography and physiological sensor monitor is triggered upon detection of the potentially medically significant cardiac event and the electrocardiographic signals are directly uploaded into an electronic medical record for the patient for review by a medical professional.\n[청구항11]\n11. A computer-implemented method, comprising:associating an activity monitor with a patient configured to sense cardiac activity data comprising heart rate or heart rhythm;paring a mobile device with the activity monitor to execute an application to detect a potentially medically significant cardiac event based on the cardiac activity data; andfitting an electrocardiography and physiological sensor monitor to a sternal region of the patient to sense electrocardiographic signals that the activity monitor is not capable of obtaining, wherein the patient's access to the electrocardiography and physiological sensor monitor is triggered upon detection of the potentially medically significant cardiac event and the electrocardiographic signals are directly uploaded into an electronic medical record for the patient for review by a medical professional.","Bardy Diagnostics, Inc.","Gust H. Bardy | Jason Felix | Jon Mikalson Bishay","A1","16-236213","2018.12.28","-","A61B-005/00","-","-","-","특허공개","[청구항1]\n 1. A computer-implemented system, comprising:an activity monitor associated with a patient and configured to sense cardiac activity data comprising heart rate or heart rhythm;a mobile device paired with the activity monitor to execute an application to detect a potentially medically significant cardiac event based on the cardiac activity data; andan electrocardiography and physiological sensor monitor fitted to a sternal region of the patient to sense electrocardiographic signals that the activity monitor is not capable of obtaining, wherein the patient's access to the electrocardiography and physiological sensor monitor is triggered upon detection of the potentially medically significant cardiac event and the electrocardiographic signals are directly uploaded into an electronic medical record for the patient for review by a medical professional.","-","-","거절","-","최종거절 발송","US","-","-","-","US, US, US","-","2019-0133444","2019.05.09","-","-","2038.12.28","-","-","2019-0133444","2019.05.09","A61B-005/00,[G16H-040/63, A61B-005/0205, A61B-005/024]","A61B-0005/0022","A61B-0005/0022, G16H-0040/0063, A61B-0005/0024, A61B-0005/0205, A61B-0005/7282, G06F-0019/0000","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","US10426364B2",1,"US(1)","US",5,165,"US2016262646A1, US9820665B2, US2017209064A1, WO2015048320A1, US2018206752A1, CA2975610C, US2016007872A1, US9408545B2, US9788722B2, US9775536B2, US10433748B2, US2018070848A1, US2017303809A1, US2017319094A1, US9737224B2, US9936875B2, US9433367B2, US2019076023A1, EP3048963B1, US2019231210A1, US10433743B1, US2016007877A1, US2017095153A1, US10052022B2, US10271755B2, US2015087948A1, US9655538B2, US9730593B2, US9554715B2, US9955885B2, US2016150989A1, US9717433B2, US2015087951A1, US2017251946A1, EP3193704B1, US2018242867A1, US9545228B2, JP2018515293A, US10478083B2, CA2982126C, US2020029842A1, JP6431624B2, US2018249924A1, US2019380615A1, EP3048954A1, EP3267881A1, US10264992B2, US2017119305A1, US10561326B2, US10278603B2, US2017135579A1, US9504423B1, US10004415B2, EP3193705B1, EP3048963A2, US2015088007A1, EP3240475A1, US2019246933A1, US9730641B2, US2018020943A1, US2016007875A1, US2018249950A1, CA2975610A1, WO2015048309A1, US2016367164A1, US10499812B2, US10251576B2, US10265015B2, WO2015048323A2, US2015087922A1, US2019380581A1, WO2015048323A3, US2016345854A1, US10278606B2, EP3193705A1, US2019231213A1, US2018220890A1, EP3536228A1, US10413205B2, US9955911B2, US2017340215A1, US9901274B2, US2019246934A1, US2017188871A1, US10271756B2, US2017196472A1, WO2016044484A1, EP3267887A1, US9717432B2, US2015087921A1, US9700227B2, US2017340206A1, US2015087950A1, US2019290150A1, US2018049640A1, US10561328B2, US2020008698A1, US9433380B1, US2016213263A1, EP3048962A1, US10154793B2, US2016278701A1, US10398334B2, US2019254553A1, US2016192853A1, US10390700B2, WO2016145392A1, US9364155B2, US2017258358A1, US9737211B2, US9345414B1, US2019133444A1, US2019117107A1, US9642537B2, WO2015048182A1, US10045709B2, US9615763B2, US10165946B2, US2020085337A1, CA2978636A1, US2017319095A1, US2016278658A1, EP3193703A1, US2017238833A1, EP3307151A1, WO2015048194A1, US2017340290A1, US2015087949A1, US2016367163A1, US10111601B2, US9655537B2, US2019239799A1, US2015088020A1, US2020037915A1, US9545204B2, US9955888B2, US10251575B2, US2015087923A1, WO2016126931A1, US2018353071A1, EP3048964A1, US2016345909A1, CA2982126A1, EP3193704A1, WO2016044477A1, US2016296166A1, US10123703B2, US2018296118A1, US2017367609A1, US2015082623A1, US2018177423A1, US2019254551A1, US10172534B2, US9619660B1, US2018344191A1, WO2016201135A1, US2019059768A1, EP3510920A1, WO2015048191A1, WO2016164623A1, US9408551B2, US2017251948A1, WO2016201118A1, WO2016044472A1, EP3048964B1","JP(2), WO(15), EP(17), US(126), CA(5)","US2019133444A1, US2015088007A1, WO2015048320A1, US10165946B2, EP3048954A1",5,"WO(1), EP(1), US(3)"]
[2,"US","System and method for controlling electrically-powered trash compactors and receptacles","Systems, methods, and computer-readable storage media for controlling electrically-powered trash compactors and receptacles. The system first receives data associated with a storage receptacle configured to communicate with the system via a network, wherein the data is received from a server storing information transmitted by the storage receptacle, the storage receptacle having an energy storage for powering operational functions performed by the storage receptacle. The system then identifies a parameter of the storage receptacle associated with an operational function of the storage receptacle, and transmits a signal to the storage receptacle for modifying the parameter based on the data associated with the storage receptacle to yield a modified operation of the storage receptacle.","[청구항1]\n1. A method comprising:transmitting, from a storage receptacle and to a network server, data collected over a first time interval by one or more sensors associated with the storage receptacle, the data corresponding to a performance of an operational function by the storage receptacle over the first time interval, the storage receptacle configured to communicate via a network, wherein the performance of the operational function is related to at least one of: compacting contents, sensing contents volume inside the storage receptacle, powering a status lamp, communicating with the network server, powering the storage receptacle, gathering weather data, gathering temperature information, running a sensor, measuring a current, detecting a movement of an item in the storage receptacle, testing a battery, and powering an advertisement display, wherein the data comprises a parameter associated with the performance of the operational function over the first time interval, wherein the parameter is related to at least one of a compaction timing, an energy usage, a timing of a sensor actuation, a desired capacity, a fullness threshold, a power mode, a fullness state, a command, a status update, an energy setting, an operating setting, a collection timing, a communication interval, a test setting, an operating current, and a compaction trigger;receiving, from the network server, a modified parameter from the network server, the modified parameter being based on the parameter associated with the performance of the operation function; andcausing, based on the modified parameter and without user intervention, a change in the storage receptacle of a performance of the operational function by the storage receptacle.\n[청구항8]\n8. A method comprising:receiving, from a storage receptacle, data collected over a first time interval by one or more sensors associated with the storage receptacle at a remote control device, the data corresponding to a performance of an operational function by the storage receptacle over the first time interval;transmitting, to the storage receptacle and from the remote control device via a network, a modification of a value of a parameter identified within the data, the parameter associated with the performance of the operational function over the first time interval, wherein the storage receptacle modifies, without manual user intervention at the storage receptacle, a future performance of the operational function by the storage receptacle according to the modification of the value of the parameter identified within the data; andreceiving, from the storage receptacle, information associated with a location of the storage receptacle for being displayed as at a particular area on at least one of a map or a list.\n[청구항14]\n14. A receptacle comprising:a processor;a transmitter for transmitting information to another device via a network;a receiver for receiving information transmitted to the receptacle via the network;a storage receptacle for storing content items; anda computer-readable storage medium having stored therein instructions which, when executed by the processor, cause the processor to perform operations comprising:transmitting data collected over a first time interval by one or more sensors associated with the storage receptacle, the data corresponding to a performance of an operational function by the storage receptacle over the first time interval, the storage receptacle configured to communicate via a network, wherein the performance of the operational function is related to at least one of: compacting contents, sensing contents volume inside the storage receptacle, powering a status lamp, communicating with the another device, powering the storage receptacle, gathering weather data, gathering temperature information, running a sensor, measuring a current, detecting a movement of an item in the storage receptacle, testing a battery, and powering an advertisement display, wherein the data comprises a parameter associated with the performance of the operational function over the first time interval, wherein the parameter is related to at least one of a compaction timing, an energy usage, a timing of a sensor actuation, a desired capacity, a fullness threshold, a power mode, a fullness state, a command, a status update, an energy setting, an operating setting, a collection timing, a communication interval, a test setting, an operating current, and a compaction trigger;receiving, from a network server, a modified parameter from the network server, the modified parameter being based on the parameter associated with the performance of the operation function; andcausing, based on the modified parameter and without user intervention, a change in the storage receptacle of a performance of the operational function by the storage receptacle.\n[청구항17]\n17. A computing device comprising:a processor;a transmitter for transmitting information to another device via a network;a receiver for receiving information transmitted to the another device via the network; anda computer-readable storage medium having stored therein instructions which, when executed by the processor, cause the processor to perform operations comprising:receiving, from a storage receptacle, data collected over a first time interval by one or more sensors associated with the storage receptacle, the data corresponding to a performance of an operational function by the storage receptacle over the first time interval;transmitting, to the storage receptacle, a modification of a value of a parameter identified within the data, the parameter associated with the performance of the operational function over the first time interval, wherein the storage receptacle modifies, without manual user intervention at the storage receptacle, a future performance of the operational function by the storage receptacle according to the modification of the value of the parameter identified within the data; andreceiving, from the storage receptacle, information associated with a location of the storage receptacle for display.","BIG BELLY SOLAR, INC.","James A. POSS | Jeffrey T. SATWICZ | Michael E. FELDMAN | David J. SKOCYPEC","A1","16-229177","2018.12.21","-","G05B-015/02","-","-","-","특허공개","[청구항1]\n 1. A method comprising:transmitting, from a storage receptacle and to a network server, data collected over a first time interval by one or more sensors associated with the storage receptacle, the data corresponding to a performance of an operational function by the storage receptacle over the first time interval, the storage receptacle configured to communicate via a network, wherein the performance of the operational function is related to at least one of: compacting contents, sensing contents volume inside the storage receptacle, powering a status lamp, communicating with the network server, powering the storage receptacle, gathering weather data, gathering temperature information, running a sensor, measuring a current, detecting a movement of an item in the storage receptacle, testing a battery, and powering an advertisement display, wherein the data comprises a parameter associated with the performance of the operational function over the first time interval, wherein the parameter is related to at least one of a compaction timing, an energy usage, a timing of a sensor actuation, a desired capacity, a fullness threshold, a power mode, a fullness state, a command, a status update, an energy setting, an operating setting, a collection timing, a communication interval, a test setting, an operating current, and a compaction trigger;receiving, from the network server, a modified parameter from the network server, the modified parameter being based on the parameter associated with the performance of the operation function; andcausing, based on the modified parameter and without user intervention, a change in the storage receptacle of a performance of the operational function by the storage receptacle.","-","-","거절","-","최종거절 발송","US","BIG BELLY SOLAR, INC.","US","-","US, US, US, US","-","2019-0113893","2019.04.18","-","-","2038.12.21","-","-","2019-0113893","2019.04.18","G05B-015/02,[B65F-001/14, B30B-009/30]","G05B-0015/0002","G05B-0015/0002, B65F-0001/1426, B30B-0009/3007, B65F-2210/0165, B65F-2210/0162, B65F-2210/0128, B65F-2210/0172, B65F-2210/0020, B65F-2210/1443","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",8,12,"US10162318B2, EP2936324A1, KR20150127572A, WO2014099190A1, US2019113893A1, EP2936324A4, JP2016502964A, AU2019232849A1, US2014172174A1, AU2013364089A1, MX2015007943A, CA2895686A1","AU(2), JP(1), KR(1), WO(1), EP(2), MX(1), US(3), CA(1)","US10162318B2, WO2014099190A1, US2019113893A1, AU2019232849A1, AU2013364089A1, CA2895686A1, EP2936324A1, KR20150127572A, EP2936324A4, JP2016502964A, US2014172174A1, MX2015007943A",12,"AU(2), JP(1), KR(1), WO(1), EP(2), MX(1), US(3), CA(1)"]
[3,"US","Activity monitors","An activity monitor that is worn by a user for monitoring water-based activities. The activity monitor includes at least one motion sensor, a water sensor, a memory, and a processor. The processor is operable to run an algorithm to calculate activity data based on an output from the motion sensor and to save the activity data to the memory. The processor can be triggered to operate to calculate the activity data and to save it to memory by an output from the water sensor to indicate that the monitor is immersed in water.","[청구항1]\n1. An activity monitor for water-based activity, the activity monitor adapted to be worn by a user to monitor a water based activity performed by the user, the monitor comprising:at least one motion sensor;a water sensor;a memory; anda processor operable to run an algorithm to calculate activity data based on an output from the at least one motion sensor and to save the activity data to the memory;wherein the processor can be triggered to operate to calculate the activity data and save it to memory by an output from the water sensor to indicate that the monitor is immersed in water.\n[청구항10]\n10. A swimsuit in combination with an activity monitor mounted on the swimsuit, wherein:the swimsuit comprises a first attachment feature at a predefined location on the suit; andthe activity monitor comprises a second attachment feature that cooperates with the first attachment features to mount the activity monitor on the swimsuit at said predefined location.","SPEEDO INTERNATIONAL LIMITED","Tim SHARPE | Depal Patel | Chris Johnson","A1","16-227762","2018.12.20","-","A61B-005/11","GB","1407288.8 ","2014.04.25","특허공개","[청구항1]\n 1. An activity monitor for water-based activity, the activity monitor adapted to be worn by a user to monitor a water based activity performed by the user, the monitor comprising:at least one motion sensor;a water sensor;a memory; anda processor operable to run an algorithm to calculate activity data based on an output from the at least one motion sensor and to save the activity data to the memory;wherein the processor can be triggered to operate to calculate the activity data and save it to memory by an output from the water sensor to indicate that the monitor is immersed in water.","-","-","심사중","-","최초거절통지 발송","GB","-","-","-","GB, GB, GB","-","2019-0125219","2019.05.02","-","-","2038.12.20","-","-","2019-0125219","2019.05.02","A61B-005/11,[G09B-019/00, A41D-007/00, A63B-069/12, G01S-019/19]","A61B-0005/1118","A61B-0005/1118, A61B-0005/1116, G09B-0019/0038, A41D-0007/0000, A63B-0069/0012, A61B-2562/0219, G01S-0019/0019, A63B-2220/0803, A61B-2503/0010, A61B-2560/0209, A63B-2244/0020, A63B-2220/0836, A61B-2560/0242, A61B-2560/0406, A61B-0005/1123","-","-","-","-","-","2014.04.25","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",7,12,"AU2015201500A1, EP3392861A1, US10201292B2, US2015305655A1, HK1217083A1, GB201407288D0, GB2528828A, EP2937849B1, JP2015208677A, EP2937849A1, CN105030243A, US2019125219A1","HK(1), AU(1), JP(1), EP(3), GB(2), CN(1), US(3)","EP3392861A1, US10201292B2, HK1217083A1, GB201407288D0, GB2528828A, EP2937849B1, JP2015208677A, EP2937849A1, US2019125219A1, AU2015201500A1, US2015305655A1, CN105030243A",12,"HK(1), AU(1), JP(1), EP(3), GB(2), CN(1), US(3)"]
[1,"JP","졸음 산출 장치","(과제) 피검사자의 현재의 활동 및 , 과거의 활동도 고려해 고정밀도로 졸음의 산출을할 수 있는 졸음 산출 장치를 제공한다. (해결수단) 스마트폰(smart phone)１에 있어서, Ｉ/Ｆ１８이 심박 센서 １９로 측정된 피검사자의 심박수 및 측정 시각을 취득하고, 상태 판별부 １１로 피검사자의 활동 상태를 판별되어 서버２으로 송신한다. 다음으로, 서버２에 있어서, 보정부 ２４으로 스마트폰(smart phone)１로부터 송신된 활동 상태에 따라 피검사자의 졸음 기준 심박수가 활동 상태마다 저장되어 있던 졸음 기준 심박 테이블 ２１로부터 졸음 기준 심박수를 취득한다. 다음으로, 보정부 ２４으로 취득한 졸음 기준 심박수를 피로도, 수면 시간, 식사한 상황에 근거하여 보정한다. 그리고, 보정한 졸음 기준 심박수(보정 졸음 기준 심박수)를 스마트폰(smart phone)１로 송신하고, 스마트폰(smart phone)１의 졸음도 산출부 １６으로 보정 졸음 기준 심박수 및 Ｉ/Ｆ１８이 취득한 심박수에 근거하여 피검사자의 졸음도를 산출한다. (선택도) 도６. ","[청구항1]\n피검사자의 심박에 관하는 생체 정보를 취득하는 생체 정보 취득부와,\n 상기 피검사자의 피로도에 관하는 피로 도 정보를 취득하는 피로 도 정보 취득부와,\n 상기 생체 정보 및 상기 피로 도 정보에 근거하여, 상기 피검사자의 현재의 졸음에 관하는 정보를 산출하는 졸음도 산출부와,\n를 구비하는 것을 특징으로 하는 졸음 산출 장치.","PIONEER ELECTRONIC CO","시모카와굉사 | 히로세지박 | 안사 미츠오","A","2018-242881","2018.12.26","-","A61B-005/16","-","-","-","특허공개","[청구항1]\n 피검사자의 심박에 관하는 생체 정보를 취득하는 생체 정보 취득부와,\n 상기 피검사자의 피로도에 관하는 피로 도 정보를 취득하는 피로 도 정보 취득부와,\n 상기 생체 정보 및 상기 피로 도 정보에 근거하여, 상기 피검사자의 현재의 졸음에 관하는 정보를 산출하는 졸음도 산출부와,\n를 구비하는 것을 특징으로 하는 졸음 산출 장치.","【課題】被検者の現在の活動及び、過去の活動をも考慮して高精度に眠気の算出をすることができる眠気算出装置を提供する。\n【解決手段】スマートフォン１において、Ｉ／Ｆ１８が心拍センサ１９で測定された被検者の心拍数及び測定時刻を取得し、状態判別部１１で被検者の活動状態を判別してサーバ２に送信する。次に、サーバ２において、補正部２４でスマートフォン１から送信された活動状態に応じて被検者の眠気基準心拍数が活動状態毎に格納されている眠気基準心拍テーブル２１から眠気基準心拍数を取得する。次に、補正部２４で取得した眠気基準心拍数を疲労度、睡眠時間、食事の状況に基づいて補正する。そして、補正した眠気基準心拍数（補正眠気基準心拍数）をスマートフォン１に送信し、スマートフォン１の眠気度算出部１６で補正眠気基準心拍数及びＩ／Ｆ１８が取得した心拍数に基づいて被検者の眠気度を算出する。\n【選択図】図６",1,"거절","Y","-","JP","-","-","下川 紘史 | 廣瀬 智博 | 安士 光男","JP, JP, JP","롱야후미오, 츠다 토시아키, 후쿠다 야스히로","2019-069207","2019.05.09","-","2018.12.26","-","2017-507282","20150326","2019-069207","2019.05.09","A61B-005/16,[A61B-005/18]","-","-","A61B-005/18","-","-","4C038","4C038PP05, 4C038PS00, 4C038PQ03","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",1,1,"JP2019069207A","JP(1)","JP2019069207A",1,"JP(1)"]
[2,"JP","전자기기","(과제) 비침습으로 간편하게 피검사자의 건강 상태를 추정할 수 있는 전자기기를 제공한다. (해결수단) 전자기기는 피검사자에게 장착된 장착부와, 피검사자의 맥파를 검출하는 센서를 포함한 센서부와, 구비해 센서부는 장착부가 피검사자에게 장착되면 피검사자의 피검부위에 접촉하고, 피검사자의 맥파에 따라 변위하는 변위부를 가진다. (선택도) 도 １２. ","[청구항1]\n피검사자에게 장착된 장착부와,\n 센서를 포함한 센서부를 구비하고,\n 상기 센서부는 상기 장착부가 상기 피검사자에게 장착된다고 상기 피검사자의 피검부위에 접촉하고, 상기 피검사자의 맥파에 따라 변위하는 변위부를 가지고,\n 상기 센서는 상기 피검사자의 맥파에 따른 상기 센서부의 각도 변화를 검출하는, 전자기기.","KYOCERA CO","안토우 히로미","A","2018-241787","2018.12.25","-","A61B-005/02","JP","2015109500 ","2015.05.29","특허공개","[청구항1]\n 피검사자에게 장착된 장착부와,\n 센서를 포함한 센서부를 구비하고,\n 상기 센서부는 상기 장착부가 상기 피검사자에게 장착된다고 상기 피검사자의 피검부위에 접촉하고, 상기 피검사자의 맥파에 따라 변위하는 변위부를 가지고,\n 상기 센서는 상기 피검사자의 맥파에 따른 상기 센서부의 각도 변화를 검출하는, 전자기기.","【課題】非侵襲で簡便に被検者の健康状態を推定することができる電子機器を提供する。\n【解決手段】電子機器は、被検者に装着される装着部と、被検者の脈波を検出するセンサを含むセンサ部と、備え、センサ部は、装着部が被検者に装着されると被検者の被検部位に接触し、被検者の脈波に応じて変位する変位部を有する。\n【選択図】図１２",13,"등록","Y","등록","JP","-","-","安島 弘美","JP","스기무라 켄지, 스기무라 히카루 상속인, 카와이 류우케이","2019-063583","2019.04.25","-","2019.04.10","2036.05.11","2017-521668","20160511","2019-063583","2019.04.25","A61B-005/02,[A61B-005/145, A61B-005/0285]","-","-","A61B-005/145","-","-","4C017, 4C038","4C017AA09, 4C017AB02, 4C017FF17, 4C017FF15, 4C017CC02, 4C017BD04, 4C017BC20, 4C017AC40, 4C017BC11, 4C038KX02, 4C038KL05, 4C038KK00, 4C038VA05, 4C038KY03, 4C038VB12","2015.05.29","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",5,8,"JP6461334B2, JPWO2016194308A1, JP2019063583A, CN107613855A, EP3305183A1, US2018146871A1, WO2016194308A1, EP3305183A4","JP(3), WO(1), CN(1), EP(2), US(1)","JP6461334B2, JPWO2016194308A1, JP2019063583A, CN107613855A, EP3305183A1, US2018146871A1, WO2016194308A1, EP3305183A4",8,"JP(3), WO(1), CN(1), EP(2), US(1)"]
[3,"JP","식사 섭취한 감시 및 조절을 행하기 위한 식기","(과제) 식사 섭취 및 옵션에서의 신체 행동한 측정을 지원하는 식사 섭취 조절 장치를 제공한다. (해결수단) 본 발명은 건강 플랫폼에 의해 사용자의 건강을 관리하는 컴퓨터 시스템으로서, 소프트웨어 지령을 실행하는 １개의 프로세서 ２４ 및 메모리-３２과, 시스템으로 통합된 １개 또는 복수의 센서를 통해 사용자의 건강 관련 행동을 적어도 하나 검출하는 건강 행동 검출 컴포넌트 ３５과, 검출된 건강 관련 유저-행동이 기술된 정보를 연락하기 위해서 1대이상의 다른 장치와의 데이터 링크를 확립하는 통신 컴포넌트 ２６과, 사용자로부터의 설정 정보를 수신하고, １개 또는 복수의 건강 관련 사항을 사용자에게 통지하는 사용자 인터페이스컴포넌트 ２８/３０을 가지는 것을 특징으로 하고 있다. (선택도) 도４. ","[청구항1]\n건강 플랫폼에 의해 사용자의 건강을 관리하는 컴퓨터 시스템으로서,\n 소프트웨어 지령을 실행하는 1개의 프로세서(24) 및 메모리-(32)와,\n 시스템으로 통합된 1개 또는 복수의 센서를 통해 사용자의 건강 관련 행동을 적어도 하나 검출하는 건강 행동 검출 컴포넌트(35/47)와,\n 검출된 건강 관련 유저-행동이 기술된 정보를 연락하기 위해서 1대이상의 다른 장치와의 데이터 링크를 확립하는 통신 컴포넌트(26)와,\n 사용자로부터의 설정 정보를 수신하고, 1개 또는 복수의 건강 관련 사항을 사용자에게 통지하는 사용자 인터페이스컴포넌트(28/30)와,\n 를 가지는 것을 특징으로 하는 시스템.\n[청구항9]\n사용자의 건강을 관리하기 위한 전자 장치로서,\n 1개 또는 복수의 전기 회로를 구비한 케이스(20)를 가지고,\n 이 케이스는 사용자의 건강 관련 행동을 검출하는 1개 또는 복수의 센서(35)를 구비하고,\n 상기 케이스는 다른 장치와 통신 연락하는 데이터 링크 장치(26)를 구비하고, 이 데이터 링크 장치는 사용자의 건강에 관련하는 추가 센서 정보를 수신하는 인터페이스를 구비한 적어도 1개의 확장부를 가지고,\n 상기 케이스는\n 1개 또는 복수의 전기 회로로 송전하는 전원장치(34)와,\n 사용자로부터의 입력을 수신하는 컨트롤 패널(28)과,\n 사용자로의 출력을 표시하는 사용자 기구 인터페이스(30)와,\n 건강 관련 행동을 행하기 위한 1개 또는 복수의 센서로부터 수신한 센서 입력을 분석하기 위한 지시를 실행하는 프로세서 장치(24)와,\n 프로세서 장치로 액세스할 수 있던 데이터와 지시 내용을 저장하도록 설정된 메모리-(32)를 구비하고 있는 것을 특징으로 하는 전자 장치.","CHRISTINE CONTANT","안녕 탄 크리스티누","A","2018-233271","2018.12.13","-","G16H-020/60","US","12/408,622 ","2009.03.20","특허공개","[청구항1]\n 건강 플랫폼에 의해 사용자의 건강을 관리하는 컴퓨터 시스템으로서,\n 소프트웨어 지령을 실행하는 1개의 프로세서(24) 및 메모리-(32)와,\n 시스템으로 통합된 1개 또는 복수의 센서를 통해 사용자의 건강 관련 행동을 적어도 하나 검출하는 건강 행동 검출 컴포넌트(35/47)와,\n 검출된 건강 관련 유저-행동이 기술된 정보를 연락하기 위해서 1대이상의 다른 장치와의 데이터 링크를 확립하는 통신 컴포넌트(26)와,\n 사용자로부터의 설정 정보를 수신하고, 1개 또는 복수의 건강 관련 사항을 사용자에게 통지하는 사용자 인터페이스컴포넌트(28/30)와,\n 를 가지는 것을 특징으로 하는 시스템.","【課題】食事摂取及びオプションでの身体行動の測定を支援する食事摂取調節装置を提供する。\n【解決手段】本発明は、健康プラットフォームによりユーザーの健康を管理するコンピューターシステムであって、ソフトウェア指令を実行する１つのプロセッサー２４及びメモリー３２と、システムに統合された１つ又は複数のセンサーを通してユーザーの健康関連行動を少なくとも一つ検出する健康行動検出コンポーネント３５と、検出された健康関連ユーザー行動が記述された情報を連絡するために一台以上の他の装置とのデータリンクを確立する通信コンポーネント２６と、ユーザーからの設定情報を受信し、１つ又は複数の健康関連事項をユーザーに通知するユーザーインターフェース・コンポーネント２８／３０と、を有することを特徴としている。\n【選択図】図４",15,"심사중","Y","-","US","-","-","コンタン クリスティーヌ","US","십거코이치, 제자환건, 마츠시타 미츠루, 창택이치로우","2019-067441","2019.04.25","-","2018.12.13","-","2017-091804","20100319","2019-067441","2019.04.25","G16H-020/60,[A61B-005/00]","-","-","G16H-020/00","-","-","5L099, 4C117","4C117XB04, 4C117XD08, 4C117XE26, 4C117XE27, 4C117XE76, 4C117XF13, 4C117XG01, 4C117XG02, 4C117XG06, 4C117XG18, 4C117XG22, 4C117XG34, 4C117XH16, 4C117XH27, 4C117XJ13, 4C117XJ46, 4C117XJ47, 4C117XL01, 5L099AA15","2009.03.20","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",7,21,"JP6143303B2, JP2017162497A, JP2012521584A, JP2015057733A, WO2010108117A3, WO2010108117A2, US9198605B2, CN105286872B, CN105286872A, US10143420B2, AU2010226443A1, US2016038082A1, JP6453938B2, EP2409272A2, CA2755781A1, EP2409272A4, CN102481120B, JP2019067441A, CN102481120A, US2019110743A1, US2010240962A1","AU(1), JP(6), WO(2), CN(4), EP(2), US(5), CA(1)","JP6143303B2, JP2017162497A, JP2012521584A, JP2015057733A, WO2010108117A3, WO2010108117A2, US9198605B2, CN105286872B, CN105286872A, US10143420B2, AU2010226443A1, US2016038082A1, JP6453938B2, EP2409272A2, CA2755781A1, EP2409272A4, CN102481120B, JP2019067441A, CN102481120A, US2019110743A1, US2010240962A1",21,"AU(1), JP(6), WO(2), CN(4), EP(2), US(5), CA(1)"]
[1,"EP","System and method for health condition monitoring","A system (1) for health condition monitoring includes a wearable device (20), a portable device (30) and a server (40). The portable device (30) is capable of communicating between the wearable device (20) and the server (40). The system (1) further includes a non-contact ECG acquisition module (21) for capturing ECG signals from a user wearing the wearable device (20), a non-contact audio acquisition module (22) for capturing a respiratory sound signal and a heart sound signal from the user wearing the wearable device (20), a first signal processing and analysis module (24) for receiving and processing the ECG signals, the respiratory sound signal and the heart sound signal to perform QRS detection, HR calculation and ECG derived RR determination, and a second signal processing and analysis module (42) for receiving and processing the ECG signals, the respiratory sound signal and the heart sound signal to perform heart sound localization, heart sound cancellation, respiratory sound restoration, and sound based RR determination.","[청구항1]\nA system (1) for health condition monitoring comprising a wearable device (20), a portable device (30) and a server (40), the portable device (30) being capable of communicating between the wearable device (20) and the server (40), the system (1) for health condition monitoring further comprising:\na non-contact ECG acquisition module (21) embedded in the wearable device (20) for capturing ECG signals from a user wearing the wearable device (20);\na non-contact audio acquisition module (22) embedded in the wearable device (20) for capturing a respiratory sound signal and a heart sound signal from the user wearing the wearable device (20);\na first signal processing and analysis module (24) embedded in the wearable device (20) and connected with the non-contact ECG acquisition module (21) for receiving and processing the ECG signals, wherein QRS detection, HR (heart rate) calculation and ECG derived RR (respiratory rate) determination are performed in the first signal processing and analysis module (24), and the first signal processing and analysis module (24) is connected with the non-contact audio acquisition module (22) for receiving and processing the respiratory sound signal and the heart sound signal; and\na second signal processing and analysis module (42) provided on the server (40) for receiving and processing the ECG signals, the respiratory sound signal and the heart sound signal uploaded by the portable device (30), wherein heart sound localization, heart sound cancellation, respiratory sound restoration, and sound based RR determination are performed in the second signal processing and analysis module (42), so as to obtain information for health condition monitoring.\n[청구항19]\nA method for health condition monitoring, comprising steps of:\n(a) providing a wearable device (20), a portable device (30) and a server (40), the wearable device (20) comprising an embedded non-contact ECG acquisition module (21), an embedded non-contact audio acquisition module (22) and an embedded first signal processing and analysis module (24), the portable device (30) being capable of communicating between the wearable device (20) and the server (40), the server (40) comprising a second signal processing and analysis module (42);\n(b) capturing ECG signals by the non-contact ECG acquisition module (21) and capturing a respiratory sound signal and a heart sound signal by the non-contact audio acquisition module (22) from the user wearing the wearable device (20);\n(c) processing the ECG signals, the respiratory sound signal and the heart sound signal by the first signal processing and analysis module (24) to perform QRS detection, HR (heart rate) calculation and ECG derived RR (respiratory rate) determination; and\n(d) processing the ECG signals, the respiratory sound signal and the heart sound signal by the second signal processing and analysis module (42) to perform heart sound localization, heart sound cancellation, respiratory sound restoration, and sound based RR determination, and thus obtaining information for health condition monitoring.\n[청구항20]\nThe method for health condition monitoring according to claim 19, further comprising a step of obtaining a final result of RR from the ECG derived RR and the sound based RR by a weighted method, where the RR from better signal quality is assigned a heavier weight.","Delta Electronics Int'l (Singapore) Pte Ltd | Nanyang Technological University","LIN | Zhiping | YEO | Yongkiang | ZHANG | Jianmin | SER | Wee | TAI | Yenpo","A1","2018-200030","2018.10.12","-","A61B-005/0408","SG","10201708876V ","2017.10.30","특허공개","[청구항1]\nA system (1) for health condition monitoring comprising a wearable device (20), a portable device (30) and a server (40), the portable device (30) being capable of communicating between the wearable device (20) and the server (40), the system (1) for health condition monitoring further comprising:\na non-contact ECG acquisition module (21) embedded in the wearable device (20) for capturing ECG signals from a user wearing the wearable device (20);\na non-contact audio acquisition module (22) embedded in the wearable device (20) for capturing a respiratory sound signal and a heart sound signal from the user wearing the wearable device (20);\na first signal processing and analysis module (24) embedded in the wearable device (20) and connected with the non-contact ECG acquisition module (21) for receiving and processing the ECG signals, wherein QRS detection, HR (heart rate) calculation and ECG derived RR (respiratory rate) determination are performed in the first signal processing and analysis module (24), and the first signal processing and analysis module (24) is connected with the non-contact audio acquisition module (22) for receiving and processing the respiratory sound signal and the heart sound signal; and\na second signal processing and analysis module (42) provided on the server (40) for receiving and processing the ECG signals, the respiratory sound signal and the heart sound signal uploaded by the portable device (30), wherein heart sound localization, heart sound cancellation, respiratory sound restoration, and sound based RR determination are performed in the second signal processing and analysis module (42), so as to obtain information for health condition monitoring.","-","-","심사중","N","-","SG","-","-","-","SG, SG, SG, SG, SG","2K Patentanwälte Blasberg Kewitz & Reichel","3476285","2019.05.01","-","-","-","-","-","3476285","2019.05.01","A61B-005/0408,[A61B-005/0452, A61B-005/08]","-","-","-","-","-","-","-","2017.10.30","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",3,4,"SG10201708876VA, EP3476285A1, EP3476285A3, US2019125263A1","SG(1), EP(2), US(1)","SG10201708876VA, EP3476285A1, EP3476285A3, US2019125263A1",4,"SG(1), EP(2), US(1)"]
[2,"EP","Wearable device capable of recognizing sleep stage and recognition method thereof","A wearable device capable of recognizing sleep stage including a processor, an electrocardiogram sensor, an acceleration sensor and an angular acceleration sensor is provided. The processor trains a neural network module. The electrocardiogram sensor generates an electrocardiogram signal. The processor analyzes the electrocardiogram signal to generate a plurality of first characteristic values. The acceleration sensor generates an acceleration signal. The processor analyzes the acceleration signal to generate a plurality of second characteristic values. The angular acceleration sensor generates an angular acceleration signal. The processor analyzes the angular acceleration signal to generate a plurality of third characteristic values. The processor utilizes the trained neural network module to perform a sleep stage recognition operation according to the first characteristic values, the second characteristic values and the third characteristic values, so as to obtain a sleep stage recognition result.","[청구항1]\nA wearable device (100) capable of recognizing sleep stage, comprising:\na processor (110), configured to train a neural network module (121);\nan electrocardiogram sensor (130), coupled to the processor (110), and configured to generate an electrocardiogram signal (ECG), wherein the processor (110) analyzes the electrocardiogram signal (ECG) to generate a plurality of first characteristic values;\nan acceleration sensor (140), coupled to the processor (110), and configured to generate an acceleration signal (AS), wherein the processor (110) analyzes the acceleration signal (AS) to generate a plurality of second characteristic values; and\nan angular acceleration sensor (150), coupled to the processor (110), and configured to generate an angular acceleration signal (ANS), wherein the processor (110) analyzes the angular acceleration signal (ANS) to generate a plurality of third characteristic values,\nwherein the processor (110) utilizes the trained neural network module (121) to perform a sleep stage recognition operation according to the first characteristic values, the second characteristic values and the third characteristic values, so as to obtain a sleep stage recognition result.\n[청구항9]\nA recognition method of sleep stage, adapted to a wearable device (100), the wearable device (100) comprising a processor (110), an electrocardiogram sensor (130), an acceleration sensor (140) and an angular acceleration sensor (150), the method comprising:\ntraining a neural network module (121) by the processor (110);\ngenerating an electrocardiogram signal (ECG) by the electrocardiogram sensor (130), and analyzing the electrocardiogram signal (ECG) by the processor (110) to generate a plurality of first characteristic values;\ngenerating an acceleration signal (AS) by the acceleration sensor (140), and analyzing the acceleration signal (AS) by the processor (110) to generate a plurality of second characteristic values;\ngenerating an angular acceleration signal (ANS) by the angular acceleration sensor (150), and analyzing the angular acceleration signal (ANS) by the processor (110) to generate a plurality of third characteristic values; and\nutilizing the trained neural network module (121) by the processor (110) to perform a sleep stage recognition operation according to the first characteristic values, the second characteristic values and the third characteristic values, so as to obtain a sleep stage recognition result.\n[청구항12]\nThe recognition method of sleep stage according to claim 11, further comprising:\nperforming an adjacent R-waves difference analysis operation by the processor (110) to analyze the heart beat interval variation (RRI) of the electrocardiogram signal (ECG), so as to obtain a mean value and a sample entropy value (EAD_mean),\nwherein the first characteristic values comprise the mean value and the sample entropy value (EAD_SE1).","Kinpo Electronics, Inc.","HARAIKAWA | Koichi | CHIEN | Jen-Chien | LIN | Yin-Tsong | HUNG | Tsui-Shan | LIN | Chien-Hung","A1","2018-183026","2018.07.11","-","A61B-005/00","TW","106140053 ","2017.11.20","특허공개","[청구항1]\nA wearable device (100) capable of recognizing sleep stage, comprising:\na processor (110), configured to train a neural network module (121);\nan electrocardiogram sensor (130), coupled to the processor (110), and configured to generate an electrocardiogram signal (ECG), wherein the processor (110) analyzes the electrocardiogram signal (ECG) to generate a plurality of first characteristic values;\nan acceleration sensor (140), coupled to the processor (110), and configured to generate an acceleration signal (AS), wherein the processor (110) analyzes the acceleration signal (AS) to generate a plurality of second characteristic values; and\nan angular acceleration sensor (150), coupled to the processor (110), and configured to generate an angular acceleration signal (ANS), wherein the processor (110) analyzes the angular acceleration signal (ANS) to generate a plurality of third characteristic values,\nwherein the processor (110) utilizes the trained neural network module (121) to perform a sleep stage recognition operation according to the first characteristic values, the second characteristic values and the third characteristic values, so as to obtain a sleep stage recognition result.","-","-","심사중","N","-","TW","-","-","-","TW, TW, TW, TW, TW","Emde, Eric","3485803","2019.05.22","-","-","-","-","-","3485803","2019.05.22","A61B-005/00,[A61B-005/0205, A61B-005/0402, A61B-005/11]","A61B-0005/4812","A61B-0005/4812, A61B-0005/0205, A61B-0005/0245, A61B-0005/0402, A61B-0005/0456, A61B-0005/1118, A61B-0005/6801, A61B-0005/7267, A61B-2562/0219, G06N-0003/0008","-","-","-","-","-","2017.11.20","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",3,3,"EP3485803A1, TW201922169A, US2019150828A1","TW(1), EP(1), US(1)","EP3485803A1, TW201922169A, US2019150828A1",3,"TW(1), EP(1), US(1)"]
[3,"EP","Wearable device capable of recognizing doze-off stage and recognition method thereof","A wearable device capable of recognizing doze-off stage including a processor and an electrocardiogram sensor is provided. The processor trains a neural network module. The processor is coupled to the electrocardiogram sensor. The electrocardiogram sensor is configured to generate an electrocardiogram signal. The processor performs a heart rate variability analysis operation and a R-wave amplitude analysis operation to analyze a heart beat interval variation of the electrocardiogram signal, so as to generate a plurality of characteristic values. The processor utilizes the trained neural network module to perform a doze-off stage recognition operation according to the characteristic values, so as to obtain a doze-off stage recognition result. In addition, a recognition method is also provided.","[청구항1]\nA wearable device (100) capable of recognizing doze-off stage, comprising:\na processor (110), configured to train a neural network module; and\nan electrocardiogram sensor (130), coupled to the processor (110), and configured to generate an electrocardiogram signal (ECG), wherein the processor (110) performs a heart rate variability analysis operation and a R-wave amplitude analysis operation to analyze a heart beat interval variation of the electrocardiogram signal (ECG), so as to generate a plurality of characteristic values,\nwherein the processor (110) utilizes the trained neural network module (121) to perform a doze-off stage recognition operation according to the characteristic values, so as to obtain a doze-off stage recognition result.\n[청구항7]\nA recognition method of doze-off stage, adapted to a wearable device (100), the wearable device (100) comprising a processor (110) and an electrocardiogram sensor (130), the method comprising:\ntraining a neural network module by the processor (110);\ngenerating an electrocardiogram signal (ECG) by the electrocardiogram sensor (130);\nperforming a heart rate variability analysis operation and a R-wave amplitude analysis operation by the processor (110) to analyze a heart beat interval variation of the electrocardiogram signal (ECG), so as to generate a plurality of characteristic values; and\nutilizing the trained neural network module (121) by the processor (110) to perform a doze-off stage recognition operation according to the characteristic values, so as to obtain a doze-off stage recognition result.","Kinpo Electronics, Inc.","HARAIKAWA | Koichi | CHIEN | Jen-Chien | LIN | Yin-Tsong | HUNG | Tsui-Shan | HSIEH | Yi-Ta | LIN | Chien-Hung","A1","2018-183027","2018.07.11","-","A61B-005/00","TW","106140054 ","2017.11.20","특허공개","[청구항1]\nA wearable device (100) capable of recognizing doze-off stage, comprising:\na processor (110), configured to train a neural network module; and\nan electrocardiogram sensor (130), coupled to the processor (110), and configured to generate an electrocardiogram signal (ECG), wherein the processor (110) performs a heart rate variability analysis operation and a R-wave amplitude analysis operation to analyze a heart beat interval variation of the electrocardiogram signal (ECG), so as to generate a plurality of characteristic values,\nwherein the processor (110) utilizes the trained neural network module (121) to perform a doze-off stage recognition operation according to the characteristic values, so as to obtain a doze-off stage recognition result.","-","-","심사중","N","-","TW","-","-","-","TW, TW, TW, TW, TW, TW","Emde, Eric","3485804","2019.05.22","-","-","-","-","-","3485804","2019.05.22","A61B-005/00,[A61B-005/024, A61B-005/0245, G06K-009/00]","A61B-0005/4809","A61B-0005/4809, A61B-0005/2405, A61B-0005/0245, A61B-0005/4012, A61B-0005/0432, A61B-0005/0456, A61B-0005/4812, A61B-0005/7267, G06K-0009/0496, G06K-0009/0516, G06K-0009/0536, G06K-0009/6273, G06N-0003/0008","-","-","-","-","-","2017.11.20","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",3,3,"US2019150827A1, TW201922170A, EP3485804A1","TW(1), EP(1), US(1)","US2019150827A1, TW201922170A, EP3485804A1",3,"TW(1), EP(1), US(1)"]
[1,"CN","Wearer identity detecting method and device and corresponding wearable device","The invention discloses a wearer identity detecting method and device and a corresponding wearable device in the technical field of wearable devices. The method includes the steps of obtaining identity feature information of a wearer when it is detected that preset detection triggering conditions are met, detecting the identity of the wearer according to the identity feature information, and conducting warning operation through a preset warning mode when the detection result shows that the identity is abnormal. By detecting the identity of the wearer of the wearable device, when the detectionresult shows that the identity is abnormal, warning operation is conducted, so the aim of monitoring the safety state of the wearer of the wearable device is realized, warning is executed to ensure the personal safety of the wearer when it is monitored that the wearer is in potential dangers, and the product monitoring and protecting strength of the wearable device on the aspect of safety of the wearer is improved.","[청구항1]\n1. A wearable device to the identification of the wearing of the detection method, characterized in that includes:When detecting the satisfies a predetermined detection when a trigger condition, obtaining of identity information;According to the identity characteristic information, to the identity of the detection;When the detection result is abnormal when the identity, by a predetermined alarm mode of the alarm operation.\n[청구항4]\n4. Any one of the method according to Claim 1-3, characterized in that the detected satisfies a predetermined detection when a trigger condition, obtaining of identity information, including:When detecting the satisfies a predetermined detection when a trigger condition, through a predetermined prompt mode, output obtaining identity information input prompt information;Obtaining based on the input prompt information input identity information.\n[청구항7]\n7. A wearable device to the identification of the wearing of the detection device, characterized in that includes:Obtaining module, for when the detected satisfies a predetermined detection when a trigger condition, obtaining of identity information;Detecting module, for in accordance with the obtaining module to said identity information, said identity of the detection;Alarm module, for when the detection module is abnormal when the identity of the detection result, the predetermined alarm mode of the alarm operation.\n[청구항9]\n9. A wearable device, characterized in that includes:The at least one processor;And with the processor connected to the at least one memory, bus; whereinThe processor, memory through the bus to accomplish the communication between each other;Said processor is used for transferring the program in the memory instruction, to the implementation of claim 1 to claim 6 any one of the identification of the device may dress the wearing of the detection method.\n[청구항10]\n10. A computer readable storage medium, characterized in that the stated computer readable storage medium storing computer instructions, the computer instructions that cause the computer implementation of the claim 1 to claim 6 any one of the identification of the device may dress the wearing of the detection method.","CHUMEN WENWEN INFORMATION TECH CO LTD","ZHANG BO","A","2018-11644130","2018.12.29","-","A61B-005/1171","-","-","-","특허공개","[청구항1]\n 1. A wearable device to the identification of the wearing of the detection method, characterized in that includes:When detecting the satisfies a predetermined detection when a trigger condition, obtaining of identity information;According to the identity characteristic information, to the identity of the detection;When the detection result is abnormal when the identity, by a predetermined alarm mode of the alarm operation. ","本发明公开了一种佩戴人身份的检测方法、装置及相应的可穿戴设备，应用于可穿戴设备技术领域。该方法包括：当检测到满足预定检测触发条件时，获取佩戴人的身份特征信息，然后根据身份特征信息，对佩戴人的身份进行检测，当检测结果为身份异常时，通过预定的告警方式进行告警操作。本发明通过检测可穿戴设备佩戴者的身份，在检测结果为身份异常时实施告警操作，实现了对可穿戴设备佩戴者的安全状态进行监测的目的，并在监测到佩戴人存在潜在危险的情况下，执行告警以保证佩戴人人身安全，提升了可穿戴设备在佩戴人安全方面的产品监控及保护力度。",10,"-","-","-","-","-","-","张博","-","-","109730690","2019.05.10","-","-","-","-","-","109730690","2019.05.10","A61B-005/1171,[A61B-005/0402, A61B-005/1172]","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",1,1,"CN109730690A","CN(1)","CN109730690A",1,"CN(1)"]
[2,"CN","Mattress for collecting sleep quality data and comparative analysis method of mattress","The invention discloses a mattress for collecting sleep quality data. A sleep monitoring module, a data storage module and a data processing module are arranged inside the mattress, the sleep monitoring module comprises a sound recording submodule and a body position monitoring submodule, the sound recording submodule is used for recording breath sound and frequency of a user in sleep, the body position monitoring submodule is used for judging body position change frequency and judges sleep conditions and body position change conditions according to the compression amount of a plurality of springs placed in the mattress, the data storage module is used for storing the breath frequency and the body position change frequency of the user in each sleep, and the data processing module is used for analyzing sleep data at night. Compared with a traditional method, the method has the advantages that the risk of radiation in the traditional method is avoided as body position change is judged bythe aid of physical deformation of the springs, the sleep data at night are compared with past data of the user, analysis is performed to obtain the sleep conditions at night, and the acquired sleepquality data are more accurate.","[청구항1]\n1. A collection sleep quality data of the mattress, including the mattress, characterized in that also includes said mattress is set in a sleep monitoring module, the sleep monitoring module for monitoring the sleep data;A data storage module, the data storage module is used for storing the sleep monitoring module sleep data;A data processing module, the data processing module is used for processing and analyzing the sleep monitoring module sleep data, and reached the conclusion that the data processing result;A warning module, the reminding module for receiving the data processing module of the data processing result, and to the data processing module of the processing of the remind.\n[청구항5]\n5. A adopts the claim 1 states the mattress in the analysis of the contrast method, characterized in that comprises the following steps of:Step A: the sleep monitoring module monitoring human sleep data, the data storage module sleep data storage, while the sleep monitoring module sleep data is transmitted to the data processing module for processing and analysis;Step B: said data processing module according to said data storage module stores the past its own sleep data comparison, determining sleep quality situation;Step C: against the data processing module judges the situation of sleep quality, the reminding module made the reminder.\n[청구항8]\n8. A collection sleep quality data of the mattress according to Claim 5, characterized in that in the step C, the reminding means including mobile phone APP application reminded.","ZHEJIANG MENGSHEN HOME CO LTD","YU TING | GUO NING","A","2018-11632921","2018.12.29","-","A61B-005/00","-","-","-","특허공개","[청구항1]\n 1. A collection sleep quality data of the mattress, including the mattress, characterized in that also includes said mattress is set in a sleep monitoring module, the sleep monitoring module for monitoring the sleep data;A data storage module, the data storage module is used for storing the sleep monitoring module sleep data;A data processing module, the data processing module is used for processing and analyzing the sleep monitoring module sleep data, and reached the conclusion that the data processing result;A warning module, the reminding module for receiving the data processing module of the data processing result, and to the data processing module of the processing of the remind. ","一种收集睡眠质量数据的床垫，床垫内部设有睡眠监测模块、数据储存模块，数据处理模块；睡眠监测模块包括声音收录子模块和体位监测子模块，声音收录子模块用于收录睡眠时的呼吸声及频率；体位监测子模块用于判定人体体位变动频率；体位监测子模块利用若干个床垫内置弹簧的压缩量判断睡眠情况和体位变动情况；数据储存模块用于储存每次睡眠的呼吸频率和体位变动频率；数据处理模块用于分析当晚睡眠数据。与传统方法相比，本发明的有益效果是：由于本发明利用弹簧物理形变判断人体体位变动，避免了传统方法中受辐射的风险，再由当晚的睡眠数据结合自身以往数据进行对比，分析得到当晚的睡眠情况，使得到的睡眠质量数据更加准确。",8,"-","-","-","-","-","-","余霆 | 郭宁","-","-","109497953","2019.03.22","-","-","-","-","-","109497953","2019.03.22","A61B-005/00,[A61B-005/08, A61B-005/11]","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",1,1,"CN109497953A","CN(1)","CN109497953A",1,"CN(1)"]
[3,"CN","Blood glucose monitoring system and method","The invention discloses a blood sugar monitoring system and method, and belongs to the field of mobile medical treatment. The monitoring system includes a data acquisition module, an information inputmodule and a data processing module. The monitoring method includes the following steps that 1, basic blood sugar information and check list information are input; 2, drug information, exercise amount and heart rate data are input; 3, input food information is recorded; 4, all the input data is analyzed and analyzed intelligently; 5, an analysis result is transmitted to a user terminal; 6, according to the data analysis result, an online appointment can be made. According to the system and the method, patients can collect information independently, a blood sugar analysis result is obtained through data analysis, the patients and doctors are informed in time, and the appointment can be made according to the data analysis result, so that the patients can obtain doctors' treatment advice intime.","[청구항1]\n1. A blood glucose monitoring system, characterized in that the system comprises a data acquisition module, the information input module and a data processing module, the data acquisition module for collecting medical original data, said information input module for manual or automatic input patient information or medical data, the data processing module is used for system automatic finishing analysis input information.\n[청구항4]\n4. The motor of claim 1 - 3 any of the blood glucose monitoring system is used for monitoring the blood sugar of the method, characterized in that comprises the following steps:S1, input blood sugar basic information and compatibility information;S2, the input medication information and exercise, the heart rate data;S3, recording the food intake information;S4, analysis of the input all data and intelligent data analysis;S5, the results of the analysis will be transmitted to the user terminal.","SUN CHENGLIN","SUN CHENGLIN","A","2018-11636571","2018.12.29","-","A61B-005/145","-","-","-","특허공개","[청구항1]\n 1. A blood glucose monitoring system, characterized in that the system comprises a data acquisition module, the information input module and a data processing module, the data acquisition module for collecting medical original data, said information input module for manual or automatic input patient information or medical data, the data processing module is used for system automatic finishing analysis input information. ","本发明公开了一种血糖监测系统及方法，属于移动医疗领域，监测系统包括数据采集模块、信息输入模块和数据处理模块，监测方法包括：S1，输入血糖基本信息以及检查单信息；S2，输入服用药物信息及运动量、心率数据；S3，记录摄入的食物信息；S4，分析输入的所有数据并进行智能的数据分析；S5，将分析的结果传输给用户终端；S6，根据数据分析结果，可以在线进行预约。使用该系统及方法可以使患者自主进行信息采集，通过数据分析得到血糖分析结果，并及时通知患者和医生，且可以根据数据分析结果进行预约，让患者及时获得医生的治疗建议。",10,"-","-","-","-","-","-","孙成林","-","-","109620252","2019.04.16","-","-","-","-","-","109620252","2019.04.16","A61B-005/145,[A61B-005/0205, A61B-005/11, G16H-050/30, G16H-080/00]","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",1,1,"CN109620252A","CN(1)","CN109620252A",1,"CN(1)"]